Back To Index << Back To Templates

# Template IPS Radiology Result Observation Component

Id | 2.16.840.1.113883.10.22.17 | Effective Date | 2024‑08‑04 20:18:47
Status | Draft | Version Label | STU2
Name | IPSRadiologyResultObservationComponent | Display Name | IPS Radiology Result Observation Component
Description
IPS Radiology Result Observation Component The component carries additional detailed radiological results. Depending on it's type the code and value have different constraints to reflect proper results.
Type of result | Constraints for `code` (Value Set) | Value Domain `value` type
Observation Text | IPS Results Radiology Textual Observations | String
Observation Code | IPS Results Radiology Observation | Code
Observation Measurement, including linear, area and volume quantity measurements | IPS Results Radiology Measurement Observation | Quantity
Observation Measurement, including linear, area and volume range measurements | IPS Results Radiology Measurement Observation | Interval of quantity
Observation Measurement, including linear, area and volume ratio measurements | IPS Results Radiology Measurement Observation | Ratio of quantity
Observation Measurement, including linear, area and volume sampled data measurements | IPS Results Radiology Measurement Observation | Sample Data (Binary)
Context | Parent nodes of template element with id 2.16.840.1.113883.10.22.17
Classification | CDA Entry Level Template
Open/Closed | Open (other than defined elements are allowed)
Used by / Uses |
Used by 0 transactions and 4 templates, Uses 0 templates
Used by | as | Name | Version
--- | --- | --- | ---
2.16.840.1.113883.10.22.4.12 | Containment | IPS Radiology Result Observation (STU2) | 2024‑08‑04 20:18:00
2.16.840.1.113883.10.22.4.9 |  | IPS Result Organizer (STU1) | 2017‑03‑02
2.16.840.1.113883.10.22.3.14 |  | IPS Results Section (STU1) | 2017‑04‑30
2.16.840.1.113883.10.22.1.2 |  | International Patient Summary (2024) | 2024‑08‑02 13:02:39
Relationship | Specialization: template 2.16.840.1.113883.10.12.303 CDA Observation (2005‑09‑07) ref ad1bbr-
Item | DT | Card | Conf | Description | Label
--- | --- | --- | --- | --- | ---
hl7:observation |  |  |  |  |
@classCode | cs | 1 … 1 | F | OBS
@moodCode | cs | 1 … 1 | R |
| CONF |
The value of @moodCode SHALL be drawn from value set 2.16.840.1.113883.1.11.18943 x_ActMoodDocumentObservation (DYNAMIC)
hl7:templateId | II | 1 … 1 | R |  |
@root | uid | 1 … 1 | F | 2.16.840.1.113883.10.12.303
hl7:id | II | 0 … * |  |  |
Choice | 1 … 1 |  | Elements to choose from: hl7:code hl7:code[concat(@code, @codeSystem) = doc('include/voc-2.16.840.1.113883.11.22.66-DYNAMIC.xml')//valueSet[1]/conceptList/concept/concat(@code, @codeSystem) or @nullFlavor] hl7:code[concat(@code, @codeSystem) = doc('include/voc-2.16.840.1.113883.11.22.80-DYNAMIC.xml')//valueSet[1]/conceptList/concept/concat(@code, @codeSystem) or @nullFlavor]
hl7:code | CE | 0 … 1 | R |  |
| CONF |
The value of @code SHALL be drawn from value set 2.16.840.1.113883.11.22.40 IPS Results Radiology Observation (DYNAMIC)
hl7:code | CE | 0 … 1 | R |  |
| CONF |
The value of @code SHALL be drawn from value set 2.16.840.1.113883.11.22.66 IPS Results Radiology Textual Observations (DYNAMIC)
hl7:code | CE | 0 … 1 | R | Codes identifying numeric measurements |
| CONF |
The value of @code SHALL be drawn from value set 2.16.840.1.113883.11.22.80 IPS Results Radiology Measurement Observation (DYNAMIC)
hl7:text | ED | 0 … 1 |  |  |
hl7:statusCode | CS | 0 … 1 |  |  |
| CONF |
The value of @code SHALL be drawn from value set 2.16.840.1.113883.1.11.15933 ActStatus (DYNAMIC)
hl7:effectiveTime | IVL_TS | 0 … 1 |  |  |
Choice | 1 … 1 |  | Elements to choose from: hl7:value[@xsi:type='ST'] hl7:value[@xsi:type='CE.IPS'] hl7:value[@xsi:type='PQ'] hl7:value[@xsi:type='IVL_PQ'] hl7:value[@xsi:type='RTO_QTY_QTY'] hl7:value[@xsi:type='BIN']
hl7:value | ST | 0 … 1 | R | Observation Text |
where [@xsi:type='ST'] |
hl7:value | CE.IPS | 0 … 1 | R | Observation Code |
where [@xsi:type='CE.IPS'] |
hl7:value | PQ | 0 … 1 | R | Observation Measurement, including linear, area and volume quantity measurements |
where [@xsi:type='PQ'] |
| Constraint | If Observation/value is a physical quantity (xsi:type="PQ"), the unit of measure SHALL be selected from ValueSet UnitsOfMeasureCaseSensitive 2.16.840.1.113883.1.11.12839 DYNAMIC
hl7:value | IVL_PQ | 0 … 1 | R | Observation Measurement, including linear, area and volume range measurements |
where [@xsi:type='IVL_PQ'] |
| Constraint | If Observation/value is a physical quantity, the unit of measure SHALL be selected from ValueSet UnitsOfMeasureCaseSensitive 2.16.840.1.113883.1.11.12839 DYNAMIC
hl7:value | RTO_QTY_QTY | 0 … 1 | R | Observation Measurement, including linear, area and volume ratio measurements |
where [@xsi:type='RTO_QTY_QTY'] |
| Constraint | If Observation/value is a physical quantity, the unit of measure SHALL be selected from ValueSet UnitsOfMeasureCaseSensitive 2.16.840.1.113883.1.11.12839 DYNAMIC
hl7:value | BIN | 0 … 1 | R | Observation Measurement, including linear, area and volume sampled data measurements |
where [@xsi:type='BIN'] |