Back To Index << Back To Terminology

# Value Set IPS Results Radiology Observation 2024‑08‑02 10:48:07

This terminology is a snapshot as of 2026‑02‑15 08:38:13. Terminologies may evolve over time. If you need recent (dynamic) versions of this terminology, please retrieve it from the source.
Id | 2.16.840.1.113883.11.22.40 | Effective Date | 2024‑08‑02 10:48:07
Canonical URI | http://hl7.org/fhir/uv/ips/ValueSet/imaging-observations-uv-ips
Status | Draft | Version Label |
Name | IPSRadResultsObservation | Display Name | IPS Results Radiology Observation
Description | Value Set Definition: LOINC {STATUS in {ACTIVE}, CLASS in LP29684-5 ("RAD")}
Usage: 2
Id | Name | Type
--- | --- | ---
Template
hl7ips-document-template- | IPS Radiology Result Observation Component (STU2) | DYNAMIC
hl7ips-entry-template-12 | IPS Radiology Result Observation (STU2) | DYNAMIC
Source Code System | 2.16.840.1.113883.6.1 - Logical Observation Identifier Names and Codes - FHIR: http://loinc.org - HL7 V2: LN
Level/ Type | Code | Intensional Definition | Code System
--- | --- | --- | ---
| Include | A valid code from the code system where: Property STATUS equal "ACTIVE" Property CLASS equal "LP29684-5" | Logical Observation Identifier Names and Codes
Legenda: Type L=leaf, S=specializable, A=abstract, D=deprecated. NullFlavor OTH (other) suggests text in originalText. HL7 V3: NullFlavors to appear in @nullFlavor attribute instead of @code.
This value set is an intensional definition that is defined by filters and rules rather than listing codes explicitly.
| XML JSON CSV SQL SVS FHIR (4.0) [xml / json]